,Air Flow Range##Other##,Static Pressure Range##Other##,Inside Duct A##Length##Inches,Fan Center M##Length##Inches,Fan Height D##Length##Inches,Model##Other##,Manufacturer##Other##,Version##Other##,Description##Other##,Unit Weight##Force##Pounds,Motor Frame Maximum Size##Other##,Leg Width L##Length##Inches,SuspensionClip Width L##Length##Inches,Outside Diameter C##Length##Inches
035A,783 to 4359(CFM),0.13 to 1.50(IN.W.G.),13.78,12,18,ATAD,Twin City Fan & Blower,0.2,TCF Axipal Tubeaxial Fan Size 035,25,145T,6.69,9.97,16.78
040A,551 to 4889(CFM),0.13 to 2.00(IN.W.G.),15.75,13,18,ATAD,Twin City Fan & Blower,0.2,TCF Axipal Tubeaxial Fan Size 040 ,37,145T,7.38,11,18.75
050A,1300 to 7491(CFM),0.13 to 1.00(IN.W.G.),19.68,15,20,ATAD,Twin City Fan & Blower,0.2,TCF Axipal Tubeaxial Fan Size 050 ,51,184T,9.25,12.94,22.68
063A,1581 to 13707(CFM),0.13 to 1.50(IN.W.G.),24.81,19,24,ATAD,Twin City Fan & Blower,0.2,TCF Axipal Tubeaxial Fan Size 063 ,104,215T,13,15.53,28.31
071A,3150 to 19861(CFM),0.13 to 2.00(IN.W.G.),27.97,20,28,ATAD,Twin City Fan & Blower,0.2,TCF Axipal Tubeaxial Fan Size 071 ,127,254T,12.75,17.13,31.47
080A,3131 to 25341(CFM),0.13 to 2.00(IN.W.G.),31.5,22,28,ATAD,Twin City Fan & Blower,0.2,TCF Axipal Tubeaxial Fan Size 080 ,191,254T,14.5,18.94,34.5
090A,7086 to 42627(CFM),0.13 to 3.00(IN.W.G.),35.44,24,36,ATAD,Twin City Fan & Blower,0.2,TCF Axipal Tubeaxial Fan Size 090 ,275,326T,16.5,20.88,38.44
100A,9221 to 55058(CFM),0.13 to 3.00(IN.W.G.),39.38,26,36,ATAD,Twin City Fan & Blower,0.2,TCF Axipal Tubeaxial Fan Size 100 ,353,326T,18.5,22.88,42.38
112A,12935 to 62912(CFM),0.13 to 3.50(IN.W.G.),44.09,29,38,ATAD,Twin City Fan & Blower,0.2,TCF Axipal Tubeaxial Fan Size 112 ,394,326T,20.75,25.22,47.09
125A,18618 to 75668(CFM),0.13 to 4.00(IN.W.G.),49.22,33,40,ATAD,Twin City Fan & Blower,0.2,TCF Axipal Tubeaxial Fan Size 125 ,465,365T,23,27.78,52.22
