,Air Flow Range##Other##,Static Pressure Range##Other##,Outside Diameter C##Length##Inches,Inside Duct A##Length##Inches,Fan Height L##Length##Inches,Model##Other##,Manufacturer##Other##,Version##Other##,Description##Other##,Unit Weight##Force##Pounds,Motor Frame Maximum Size##Other##,Leg Height E##Length##Inches,Leg Length G##Length##Inches
035A,783 to 4359(CFM),0.13 to 1.50(IN.W.G.),16.78,13.78,18,ATAD,Twin City Fan & Blower,0.2,TCF Tubeaxial Fan Size 035,25,145T,5.68,6.09
040A,551 to 4889(CFM),0.13 to 2.00(IN.W.G.),18.75,15.75,18,ATAD,Twin City Fan & Blower,0.2,TCF Tubeaxial Fan Size 040 ,37,145T,5.68,6.09
050A,1300 to 7491(CFM),0.13 to 1.00(IN.W.G.),22.68,19.68,20,ATAD,Twin City Fan & Blower,0.2,TCF Tubeaxial Fan Size 050 ,51,184T,5.68,6.27
063A,1581 to 13707(CFM),0.13 to 1.50(IN.W.G.),28.31,24.81,24,ATAD,Twin City Fan & Blower,0.2,TCF Tubeaxial Fan Size 063 ,104,215T,7.68,6.16
071A,3150 to 19861(CFM),0.13 to 2.00(IN.W.G.),31.47,27.97,28,ATAD,Twin City Fan & Blower,0.2,TCF Tubeaxial Fan Size 071 ,127,254T,7.68,6.24
080A,3131 to 25341(CFM),0.13 to 2.00(IN.W.G.),34.5,31.5,28,ATAD,Twin City Fan & Blower,0.2,TCF Tubeaxial Fan Size 080 ,191,254T,7.56,6.69
090A,7086 to 42627(CFM),0.13 to 3.00(IN.W.G.),38.44,35.44,36,ATAD,Twin City Fan & Blower,0.2,TCF Tubeaxial Fan Size 090 ,275,326T,7.56,6.6
100A,9221 to 55058(CFM),0.13 to 3.00(IN.W.G.),42.38,39.33,36,ATAD,Twin City Fan & Blower,0.2,TCF Tubeaxial Fan Size 100 ,353,326T,7.56,6.68
112A,12935 to 62912(CFM),0.13 to 3.50(IN.W.G.),47.09,44.09,38,ATAD,Twin City Fan & Blower,0.2,TCF Tubeaxial Fan Size 112 ,394,326T,9.56,6.57
125A,18618 to 75668(CFM),0.13 to 4.00(IN.W.G.),52.22,49.22,40,ATAD,Twin City Fan & Blower,0.2,TCF Tubeaxial Fan Size 125 ,465,365T,11.56,6.5
