,Air Flow Range##other##,Static Pressure Range##other##,Curb Cap SQ##Length##Inches,Shroud Overall Diameter##Length##Inches,Model##other##,Manufacturer##other##,Version##other##,Description##other##,Unit Weight##Force##pounds,Motor Housing Band Height##Length##Inches,Motor Housing Band Radius##Length##Inches,Shroud Bottom Radius##Length##Inches,Shroud Height##Length##Inches,Shroud Contour Radius##Length##Inches,Shroud Contour Radius Height##Length##Inches,Conduit Height##Length##Inches,Curb Cap Half##Length##Inches,Roof Opening Half##Length##Inches,Duct Width##Length##Inches,Duct Height##Length##Inches,Wall Bracket OD Half##Length##Inches
071B,91 to 224 (CFM),0 to 0.125 (in W.G.),17,22,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 071,100,24.44,7.5625,7.5625,18,5,8.53,10.95,8.5,5.25,10.5,10.5,8.375
072B,211 to 292 (CFM),0 to 0.125 (in W.G.),17,22,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 072,100,24.44,7.5625,7.5625,18,5,8.53,10.95,8.5,5.25,10.5,10.5,8.375
073B,275 to 439 (CFM),0 to 0.375 (in W.G.),17,22,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 073,100,24.44,7.5625,7.5625,18,5,8.53,10.95,8.5,5.25,10.5,10.5,8.375
081B,80 to 259 (CFM),0 to .0125 (in W.G.),17,22,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 081,100,24.44,7.5625,7.5625,18,5,8.53,10.95,8.5,5.25,10.5,10.5,8.375
082B,334 to 496 (CFM),0 to .025 (in W.G.),17,22,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 082,100,24.44,7.5625,7.5625,18,5,8.53,10.95,8.5,5.25,10.5,10.5,8.375
083B,418 to 780 (CFM),0 to 0.75 (in W.G.),17,22,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 083,100,24.44,7.5625,7.5625,18,5,8.53,10.95,8.5,5.25,10.5,10.5,8.375
091B,463 to 656 (CFM),0 to 0.125 (in W.G.),20,22,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 091,120,26.125,7.5625,7.5625,18,5,8.53,12.64,10,7.25,14.5,14.5,9.875
092B,307 to 836 (CFM),0 to 0.375 (in W.G.),20,22,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 092,120,26.125,7.5625,7.5625,18,5,8.53,12.64,10,7.25,14.5,14.5,9.875
093B,597 to 1307 (CFM),0 to 0.75 (in W.G.),20,22,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 093,120,26.125,7.5625,7.5625,18,5,8.53,12.64,10,7.25,14.5,14.5,9.875
110B,537 to 1638 (CFM),0 to 1.25 (in W.G.),24,30,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 110,135,28.3125,10,11,28,9,11,14.33,12,8.75,17.5,17.5,11.875
120B,691 to 2256 (CFM),0 to 1.50 (in W.G.),24,30,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 120,135,27.19,10,11,28,9,11,13.7,12,8.75,17.5,17.5,11.875
140B,1155 to 2261 (CFM),0 to 0.75 (in W.G.),24,30,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 140,145,27.68,10,11,28,9,11,14.2,12,8.75,17.5,17.5,11.875
160B,1380 to 2923 (CFM),0 to 1.00 (in W.G.),24,30,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 160,180,29.8125,10,11,28,9,11,16.33,12,8.75,17.5,17.5,11.875
180B,1550 to 3865 (CFM),0 to 1.25 (in W.G.),30,36,DCRWR,Twin City Fan & Blower,0.4,TCF Restuarant Wall Exhauster Direct Driven size 180,180,29.17,12,11.94,30,9,13.4,15.7,15,12.25,24.5,24.5,14.875
