,Air Flow Range##Other##,Static Pressure Range##Other##,Model##Other##,Manufacturer##Other##,Version##Other##,Description##Other##,Unit Weight##Force##Pounds,Motor Frame Maximum Size##Other##,Outside Flange C##Length##Inches,Inside Duct A##Length##Inches,Housing D##Length##Inches,Frame Width_S##Length##Inches,Motor Dia_P##Length##Inches,Motor Shaft Dia_U##Length##Inches,Motor Shaft Length_N##Length##Inches
12,730 to 1953(CFM),0 to 0.88(IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 12,51,145T,14.88,12.25,12,7.5,6.63,0.88,2.5
14,1691 to 2991(CFM),0 to 0.88(IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 14,56,145T,16.88,14.25,12,7.5,6.63,0.88,3.56
16,1815 to 3709(CFM),0 to 1.13(IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 16,61,184T,19,16.25,12,8,7.88,1.13,3.56
18,2320 to 5684(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 18,61,184T,21,18.25,12,8,7.88,1.13,3.56
24,5574 to 9488(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 24,119,184T,27.13,24.25,15.5,8.5,7.88,1.13,3.56
30,5537 to 16104(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 30,134,184T,33.25,30.38,15.5,13.5,7.88,1.13,3.56
34,9176 to 20567(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 34,139,184T,37.38,34.38,15.5,13.5,7.88,1.13,3.56
36,10767 to 22684(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 36,164,184T,39.38,36.38,15.5,13.5,7.88,1.13,3.56
42,14918 to 36131(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 42,194,215T,45.5,42.5,15.5,13.5,9.56,1.38,3.88
