,Air Flow Range##Other##,Static Pressure Range##Other##,Model##Other##,Manufacturer##Other##,Version##Other##,Description##Other##,Unit Weight##Force##Pounds,Motor Frame Maximum Size##Other##,Motor Diameter P##Length##Inches,Shaft Diameter U##Length##Inches,Shaft Length N##Length##Inches,Frame Width S##Length##Inches,Leg Width L##Length##Inches,Leg Height E##Length##Inches,Leg Cut S##Length##Inches,Housing Radius V##Length##Inches,Housing Offset AA##Length##Inches,Outside Flange C##Length##Inches,Inside Duct A##Length##Inches,Housing D##Length##Inches
12,730 to 1953(CFM),0 to 0.88(IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 12,51,145T,6.63,0.88,2.5,7.5,14.75,7.12,1.25,6.41,11.63,14.88,12.25,12
14,1691 to 2991(CFM),0 to 0.88(IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 14,56,145T,6.63,0.88,3.56,7.5,17.5,7.49,2,7.41,12.38,16.88,14.25,12
16,1815 to 3709(CFM),0 to 1.13(IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 16,61,184T,7.88,1.13,3.56,8,19,7.12,2.09,8.41,13.38,19,16.25,12
18,2320 to 5684(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 18,61,184T,7.88,1.13,3.56,8,21,8.41,2.25,9.41,15.63,21,18.25,12
24,5574 to 9488(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 24,119,184T,7.88,1.13,3.56,8.5,28,10.25,2.75,12.28,17.75,27.13,24.25,15.5
30,5537 to 16104(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 30,134,184T,7.88,1.13,3.56,13.5,34,12.125,3.25,15.34,21.31,33.25,30.38,15.5
34,9176 to 20567(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 34,139,184T,7.88,1.13,3.56,13.5,39,14.125,3.88,17.5,24,37.38,34.38,15.5
36,10767 to 22684(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 36,164,184T,7.88,1.13,3.56,13.5,42,15.41,4.125,18.53,25.25,39.38,36.38,15.5
42,14918 to 36131(CFM),0 to 1.25IN.W.G.),TCBS,Twin City Fan & Blower,0.2,TCF Paint Booth Exhaust Tubeaxial Fan Size 42,194,215T,9.56,1.38,3.88,13.5,46,14.47,3.875,21.75,27.5,45.5,42.5,15.5
