,Air Flow Range##Other##,Static Pressure Range##Other##,Model##Other##,Manufacturer##Other##,Version##Other##,Description##Other##,Motor Frame Maximum Size##Other##,Unit Weight##Force##Pounds,Outside Diameter C##Length##Inches,Fan Height A##Length##Inches,Inside Duct B##Length##Inches
12 D7,1750 to 3500(CFM),0.25 to 3.00(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 12 D7,140C,25,15.16,24.5,12.16
15 D6,1750 to 3500(CFM),0.25 to 4.00(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 15 D6,140C,37,18.16,27,15.15
15 D7,1750 to 3500(CFM),0.25 to 5.00(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 15 D7,180C,51,18.16,27,15.16
18 D5,1170 to 1750(CFM),0.25 to 1.00(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 18 D5,140C,104,21.16,24.5,18.16
18 D6,1170 to 1750(CFM),0.25 to 1.25(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 18 D6,180C,127,21.16,28,18.16
18 D7,1170 to 3500(CFM),0.25 to 5.00(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 18 D7,210C,191,21.16,28,18.16
21 D4,880 to 1750(CFM),0.25 to 1.25(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 21 D4,140C,275,24.19,27,21.19
21 D5,880 to 1750(CFM),0.25 to 1.50(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 21 D5,180C,353,24.19,27,21.19
21 D6,880 to 1750(CFM),0.25 to 1.50(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 21 D6,210C,394,24.19,32,21.19
24 D4,880 to 1750(CFM),0.25 to 1.50(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 24 D4,180C,502,27.19,28,24.19
24 D5,880 to 1750(CFM),0.25 to 2.00(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 24 D5,210C,551,27.19,28,24.19
28 D4,880 to 1750(CFM),0.25 to 2.00(IN.W.G.),TCVA,Twin City Fan & Blower,0.2,TCF Vaneaxial  Fan Size 28 D4,210C,610,31.25,32,28.25
