,Air Flow Range##Other##,Static Pressure Range##Other##,Model##Other##,Manufacturer##Other##,Version##Other##,Description##Other##,Unit Weight##Force##Pounds,Motor Frame Maximum Size##Other##,Fan Diameter F##Length##Inches,Fan Plate C##Length##Inches,Square Panel A##Length##Inches,Frame Dimension_G##Length##Inches,Motor Length_L##Length##Inches,Motor Diameter##Length##Inches,Motor Shaft Diameter U##Length##Inches,Motor Shaft Length V##Length##Inches,Wall Box K##Length##Inches,Wall Box Width J1##Length##Inches,Motor Side Wire Guard H##Length##Inches,Motor Operated Shutter J2##Length##Inches,Motor Operated Shutter A##Length##Inches,Motor Side Guard B##Length##Inches,Gravity Shutter A##Length##Inches,Fan Plate D##Length##Inches,WH Wall Box Mount A##Length##Inches,WH Wall Mount A##Length##Inches,Weather Hood B##Length##Inches
24DE4,1643 to 10932(CFM),0 to 1.00(IN.W.G.),TCWPX,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 24,90,215T,24,5,30,20.63,0.5,9.56,1.38,3.38,30.25,13.5,29,24,30.25,30.13,30.25,2.75,30.25,34.38,28
30DE4,4534 to 22012(CFM),0 to 1.50(IN.W.G.),TCWPX,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 30,125,215T,30,5.63,36,23.38,0.5,9.56,1.38,3.38,36.25,14,31.75,24,36.25,36.13,36.25,2.75,36.25,39.63,33.25
36DE4,4695 to 33864(CFM),0 to 1.50(IN.W.G.),TCWPX,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 36,180,215T,36,5.5,42,23.25,0.5,9.56,1.38,3.38,42.25,14,31.63,26,42.25,42.13,42.25,2.75,42.25,45.63,39.25
42DE4,9873 to 58508(CFM),0 to 1.50(IN.W.G.),TCWPX,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 42,265,256T,42,5.5,48,27.5,0.5,12.94,1.63,4,48.25,14,35.88,26,48.25,48.13,48.25,2.75,48.25,51.63,45.25
48DE4,12354 to 53667(CFM),0 to 1.50(IN.W.G.),TCWPX,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 48,375,286T,48,6,54,31.25,0.5,14.63,1.88,4.63,54.25,16,39.63,26,54.25,54.13,54.25,2.75,54.25,57.63,51.25
