,Air Flow Range##Other##,Static Pressure Range##Other##,Model##Other##,Manufacturer##Other##,Version##Other##,Description##Other##,Unit Weight##Force##Pounds,Motor Frame Maximum Size##Other##,Fan Diameter F##Length##Inches,Fan Plate C##Length##Inches,Square Panel A##Length##Inches,Propeller Width G##Length##Inches,Motor Length##Length##Inches,Motor Diameter##Length##Inches,Motor Shaft Diameter U##Length##Inches,Motor Shaft Length V##Length##Inches,Wall Box K##Length##Inches,Wall Box Width J1##Length##Inches,Motor Side Wire Guard H##Length##Inches,Motor Operated Shutter J2##Length##Inches,Motor Operated Shutter A##Length##Inches,Motor Side Guard B##Length##Inches,Gravity Shutter A##Length##Inches,WH Wall Box Mount A##Length##Inches,WH Wall Mount A##Length##Inches,Weather Hood B##Length##Inches,WH Wall Box Mount A##Length##Inches,WH Wall Mount A##Length##Inches,Weather Hood B##Length##Inches
24BTC,3600 to 12000(CFM),0 to 1.50(IN.W.G.),TCWP,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 24,115,145T,24.38,7.75,30,20.75,12.55,6.63,0.88,2.25,30.25,13.5,27.37,24,30.25,30.13,30.25,30.25,34.38,28,30.25,34.38,28
30BTC,6000 to 23000(CFM),0 to 1.50(IN.W.G.),TCWP,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 30,170,184T,30.25,8.38,36,26.75,13.76,7.88,1.13,2.75,36.25,14,33.38,24,36.25,36.13,36.25,36.25,39.63,33.25,36.25,39.63,33.25
36BTC,7000 to 26000(CFM),0 to 1.50(IN.W.G.),TCWP,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 36,220,215T,36.13,8.25,42,26.63,17.91,9.56,1.38,3.38,42.25,14,32.75,26,42.25,42.13,42.25,42.25,45.63,39.25,42.25,45.63,39.25
42BTC,9000 to 34000(CFM),0 to 1.50(IN.W.G.),TCWP,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 42,315,215T,42.5,8.25,48,26.13,17.91,9.56,1.38,3.38,48.25,14,32.25,26,48.25,48.13,48.25,48.25,51.63,45.25,48.25,51.63,45.25
48BTC,9000 to 38000(CFM),0 to 1.50(IN.W.G.),TCWP,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 48,430,256T,48.5,8.75,54,32,23.16,12.94,1.63,4,54.25,16,38.25,26,54.25,54.13,54.25,54.25,57.63,51.25,54.25,57.63,51.25
