,Air Flow Range##Other##,Static Pressure Range##Other##,Model##Other##,Manufacturer##Other##,Version##Other##,Description##Other##,Unit Weight##Force##Pounds,Motor Frame Maximum Size##Other##,Fan Diameter F##Length##Inches,Fan Plate C##Length##Inches,Square Panel A##Length##Inches,Frame Dimension_G##Length##Inches,Motor Length_L##Length##Inches,Motor Diameter##Length##Inches,Motor Shaft Diameter U##Length##Inches,Motor Shaft Length V##Length##Inches,Wall Box K##Length##Inches,Wall Box Width J1##Length##Inches,Motor Side Wire Guard H##Length##Inches,Motor Operated Shutter J2##Length##Inches,Motor Operated Shutter A##Length##Inches,Motor Side Guard B##Length##Inches,Gravity Shutter A##Length##Inches,Fan Plate D##Length##Inches,WH Wall Box Mount A##Length##Inches,WH Wall Mount A##Length##Inches,Weather Hood B##Length##Inches
24,4001 to 9744(CFM),0 to 0.88(IN.W.G.),TCWPZ,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 24,90,215T,24,7.75,30,20.75,0.5,9.56,1.38,3.38,30.25,13.5,29,24,30.25,30.13,30.25,2.75,30.25,34.38,28
30,5709 to 20029(CFM),0 to 1.50(IN.W.G.),TCWPZ,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 30,125,215T,30,8.38,36,26.13,0.5,9.56,1.38,3.38,36.25,14,31.75,24,36.25,36.13,36.25,2.75,36.25,39.63,33.25
36,9286 to 26164(CFM),0 to 1.50(IN.W.G.),TCWPZ,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 36,180,215T,36,8.25,42,26,0.5,9.56,1.38,3.38,42.25,14,31.63,26,42.25,42.13,42.25,2.75,42.25,45.63,39.25
42,9944 to 35670(CFM),0 to 1.50(IN.W.G.),TCWPZ,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 42,265,256T,42,8.25,48,26,0.5,12.94,1.63,4,48.25,14,35.88,26,48.25,48.13,48.25,2.75,48.25,51.63,45.25
48,19148 to 39986(CFM),0 to 1.25(IN.W.G.),TCWPZ,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 48,375,286T,48,8.75,54,31.25,0.5,14.63,1.88,4.63,54.25,16,39.63,26,54.25,54.13,54.25,2.75,54.25,57.63,51.25
54,Consult Factory,Consult Factory,TCWPZ,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 54,430,286T,54,8.75,60,33.25,0.5,14.63,1.88,4.63,60.25,16,39.5,26,60.25,60.13,60.25,2.75,60.25,63.63,57.25
60,Consult Factory,Consult Factory,TCWPZ,Twin City Fan & Blower,0.2,Propeller Wall Fan Size 60,505,286T,60,8.75,66,33.25,0.5,14.63,1.88,4.63,66.31,16,39.25,26,66.31,66.19,66.31,2.75,66.25,69.63,63.25
