,Air Flow Range##other##,Static Pressure Range##other##,Motor Frame Maximum Size##other##,Base Width##length##inches,Base Length##length##inches,Base Height##length##inches,Filter Box Length##length##inches,Base Weight##Force##pounds,Filter Box Weight##Force##pounds,Model##other##,Manufacturer##other##,Version##other##,Description##other##,Inlet and Outlet Width##length##inches,Inlet and Outlet Height##length##inches,Duct Length##length##inches,Inlet and Outlet Duct Width##length##inches,Inlet and Outlet Duct Height##length##inches,Side Outlet Width Half##length##inches,Side Outlet Height Half##length##inches,Side Duct Width##length##inches,Side Duct Height##length##inches
080A,232 to 620 (CFM),0 to 0.75 (in W.G.),56,15.33,19,15.33,26.63,93,18,DSI,Twin City Fan & Blower,0.7,TCF Duct Blower-square inline direct drive size 080,11.88,11.88,1,12,12,5.94,5.94,12,12
090A,390 to 950 (CFM),0 to 0.75 (in W.G.),56,15.33,19,15.33,26.63,96,15,DSI,Twin City Fan & Blower,0.7,TCF Duct Blower-square inline direct drive size 090,11.88,11.88,1,12,12,5.94,5.94,12,12
100A,520 to 1601 (CFM),0 to 1.25 (in W.G.),56,17.81,20.5,17.81,26.75,106,29,DSI,Twin City Fan & Blower,0.7,TCF Duct Blower-square inline direct drive size 100,13.88,13.88,1,14,14,6.94,6.94,14,14
120A,586 to 2132 (CFM),0 to 1.50 (in W.G.),56,19.38,21.5,19.38,30.5,127,24,DSI,Twin City Fan & Blower,0.7,TCF Duct Blower-square inline direct drive size 120,15.88,15.88,1,16,16,7.94,7.94,16,16
135A,1041 to 2924 (CFM),0 to 1.75 (in W.G.),145T,21.56,23,21.56,30,132,29,DSI,Twin City Fan & Blower,0.7,TCF Duct Blower-square inline direct drive size 135,17.88,17.88,1,18,18,8.94,8.94,18,18
135AN,670 to 2118 (CFM),0 to 2.00 (in W.G.),145T,21.56,23,21.56,30,132,29,DSI,Twin City Fan & Blower,0.7,TCF Duct Blower-square inline direct drive size 135,17.88,17.88,1,18,18,8.94,8.94,18,18
150A,1286 to 3892 (CFM),0 to 2.00 (in W.G.),145T,23.82,24,23.82,30,157,43,DSI,Twin City Fan & Blower,0.7,TCF Duct Blower-square inline direct drive size 150,19.88,19.88,1,20,20,9.94,9.94,20,20
150AN,810 to 2818 (CFM),0 to 2.00 (in W.G.),145T,23.82,24,23.82,30,157,43,DSI,Twin City Fan & Blower,0.7,TCF Duct Blower-square inline direct drive size 150,19.88,19.88,1,20,20,9.94,9.94,20,20
165A,1773 to 5898 (CFM),0 to 2.00 (in W.G.),182T,26.5,26,26.5,28,167,65,DSI,Twin City Fan & Blower,0.7,TCF Duct Blower-square inline direct drive size 165,22.88,22.88,1,23,23,11.44,11.44,23,23
165AN,1248 to 4261 (CFM),0 to 2.00 (in W.G.),182T,26.5,26,26.5,28,167,65,DSI,Twin City Fan & Blower,0.7,TCF Duct Blower-square inline direct drive size 165,22.88,22.88,1,23,23,11.44,11.44,23,23
